;---------------------------------------------------------------;
;  Windows Driver Installer
;
;  Logic Controls programmable PS2 keyboard Driver
;  for Windows Vista/XP/7/8 X86/X64
;
;  Driver type: WDM
;  01-19-2015
;---------------------------------------------------------------;

To program the KB9000 with PS/2 interface, a driver has to be
installed on the computer running the programming utility.
Please following procedure below to install the driver before
running the programming utility.


Installation Procedure
======================

1. Turn off power of computer.

2. Plug KB9000 in PS/2 port, and turn on computer power.

3. Double click on <install.bat> to install device driver 
   package automatically and wait until installation is complete.

   or,

   Double click on "LciKb_x86.msi" or "LciKb_x86.msi" directly 
   to install device driver package. Follow the instructions on 
   screen step by step to finish installation.  There are two 
   installation programs for 16 bit (x86) and 64bit (x64) 
   Windows XP/Vista/7/8.  The correct one must be used for 
   installation. If a wrong installation file is selected, 
   the installation will fail.

4. Restart computer after the installation is finished.

5. Check under Device Manager whether the device driver installed
   correctly under Keyboards device class.






Bematech / Logic Controls, Inc.
999 S. Oyster Bay Rd
Building #104
Bethpage, NY 11714
USA

Tel: +1 516 248 0400
Fax: +1 516 495 4075
www.bematechus.com
