;---------------------------------------------------------------;
;  Logic Controls, Inc. - A Bematech Company
;  Line Display LD1000
;  Firmware and Utility
;
;  10-08-2013
;  Version: V1.14
;---------------------------------------------------------------;
;  
;  Peter Li
;  Logic Controls, Inc.
;  email: pli@logiccontrols.com
;  
==============================================================================
Firmware:
;---------------------------------------------------------------;
1. <ld1d_114.hex> is the boot section firmware with LCI command set, 
   which must be written into board with Atmel programming tool. This 
   firmware program must be written into board first, then all other 
   command sets can be downloaded through communication port.

2. <LCI_114.c1f> is Logic Controls command set file, including Logic
   Controls OPOS command set.

3. <Aedex_114.c1f> is Aedex command set.

4. <Noritaki_114.c1f> is NORITAKI command set.

5. <PD3400_114.c1f> is backward compatible to PD3400 command set.

6. <utcs1100_114.c1f> is Ultimate1100XLT command set with start
   direct to pole mode.

7. <utce1100_114.c1f> is Ultimate1100XLT command set with start
   pass-through mode.

8. <Epson110_114.c1f> is Epson D-110/D202II command set.

9. <PTC7220_114.c1f> is Partner Tech CD7220 command set.

10. <emax_114.c1f> is EMAX command set.

11. <IEE_114.c1f> is IEE SP-322 command set.

12. <Firich_114.c1f> is Firich command set.

*** use <UpdateLd1Fmwr.exe> for the above 2. -- 12. downloading
==============================================================================
Utility:
;---------------------------------------------------------------;
1. Windows utility <UpdateLd1Fmwr.exe> is for downloading/updating other
   command set files into the device.

2. Make the device power off/on before downloading any command set into
   the device to avoid wrong operation of the device.
==============================================================================
