LOGIC CONTROLS USB CASH DRAWER DRIVER INSTALLATION
===================================================

5/08/2009

;---------------------------------------------------------------;
;  Windows Installer
;  Logic Controls Cash Drawer USB Devices Driver
;  for Windows Vista/XP X86/X64
;
;  Model: with USB interface
;  Driver type: Virtual COM port
;  05-05-2009
;---------------------------------------------------------------;


This driver package for Logic Controls USB Cash Drawers contains USB drivers 
for Windows XP/Vista 32bit and 64bit.  Following cash drawer models are 
supported by the USB driver:

	CR1003
	CR1603
	CR1803
	CR3003

Follow the installation instructions below carefully.



-------------------------------
WINDOWS USB DRIVER INSTALLATION
-------------------------------

1. Plug the device in USB port.

2. Double click on <install.bat> to install Cash Drawer driver
   software package quitely and wait until the installation completes.
   or,
   Double click <lcicrusb-x86.msi> / <lcicrusb-x64.msi> (depends on 
   Windows platform being used) directly to install Cash Drawer driver
   package Follow the instructions step by step to finish installation.

3. Invoke "Device Manager".

4. In Device Manager, check the COM port number under entry Ports(COM&LPT).
   The POS software will have to set up to use this COM port number for 
   operation with the Cash Drawer.


-----------------------------------------------------
Change COM port number with "Virtual COM Port Driver"
-----------------------------------------------------

1. Keep the device plugged in the USB port.

2. Invoke Device Manager.

3. Right click "LCI Cash Drawer with USB port (COMx)" under Ports(COM & LPT) 
   item and a pop up menu will be displayed.

4. Select [Properties].  A "Properties" box will be displayed.

5. Select [Port Settings] tab and click [Advanced...] button.

6. Click COM port number box to select unused port number.

7. Click <OK> buttons twice.

8. Unplug the USB cash drawer for a few seconds and then reconnect the cash 
   drawer to the USB port. Wait for the device driver to load automatically. 
   The COM port number will be updated.




-----------------------------------
SETTING UP CASH DRAWER OPENING CODE
-----------------------------------

(See section below for setup of codes for OPOS)

1.  With Windows Explorer, double click on the file "CRedit" to start 
    the utiltiy software.

2.  Select COM port name on the utility start up screen as shown under 
    Device Manager and click OK.

3.  Enter number of bytes to be used for the opening code in the "Bytes 
    in command" box (1 to 5).

4.  Enter the decimal code values in the boxes Cmd Code1 to Cmd Code5.  
    For example, enter '7' for "Ctrl-G" to open the drawer.  If the code 
    is less than 5 bytes, codes in the additional boxes will be ignored.

6.  Click "Write to CR" button to write settings to the cash drawer.

7.  Set up the POS retail software with same opening code and COM port 
    name for the cash drawer.

8.  Test with the POS retail software.

Note: For security reason, it's recommended that the programming utility 
      software should not be copied onto the cashier station computer to 
      avoid unauthorized change of the opening codes.



------------------------------------------------
SETTING UP CASH DRAWER TO WORK WITH OPOS DRIVERS
------------------------------------------------

If the POS application software works with OPOS, please install the 
Logic Controls cash drawer OPOS driver.  The latest version of OPOS
driver can be downloaded from our web site.  The cash drawer also has 
to be programmed to OPOS mode.

1.  With Windows Explorer, double click on the file "CRedit" to start 
    the utility software.

2.  Select COM port name on the utility start up screen as shown under 
    Device Manager and click OK.

3.  Check the checkbox for "OPOS/JPOS".

4.  Click "Write to CR" button to write settings to the cash drawer.

5.  In OPOS driver setup, set the COM port name, LDN and test opening the 
    drawer (refer to OPOS driver installation instructions for details).

6.  Setup POS software to to use the LDN defined in OPOS setup.

7.  Test with the POS retail software.

Note: After OPOS mode is enabled, the drawer can only be opened through
      the OPOS driver.  It will no longer response to the normal opening
      codes.





Logic Controls, Inc.
355 Denton Avenue
New Hyde Park, NY 11040
Tel: (516)-248 0400
Fax: (516)-248 0443
email: lci@logiccontrols.com
web: www.logiccontrols.com
