LOGIC CONTROLS, INC.
A Bematech Company



POS for .Net Driver for Line Displays with USB Port

===================================================



01-29-2010




This POS for .net driver supports Logic Controls OPOS USB pole 

displays and table displays.  Following models are supported:



	LD9900U		PD3900U		PD6900U

	LD9900UP	PD3900UP	PD6900UP

	LT9900U		TD3900U	               LD1000

	LT9900UP	TD3900UP

	LD9800U		PD3800U

	LD9800UP	PD3800UP

	LT9800U		TD3800U

	LT9800UP	TD3800UP



Please make sure that the line display being used is one of the 

above models.  This version of POS for .net drier only supports

USB interface line displays.  For models PD3800, TD3800, LD9800 

and LT9800, make sure that LCI command set is loaded into the display.



The following instructions are for installing Logic Controls 

POS for .Net drivers for USB Line Displays.



There are two types of USB drivers available for Logic Controls

USB display - Device Name driver and Virtual COM port driver.

The device name driver use a specific name (\\.\LCLD9, \\.\LCPD6\, 

and \\.\LCPD3\) to access the pole display directly.  Install this 

USB driver in order to work with the POS for .Net driver.









DRIVER INSTALLATION

-------------------



1.	Download Microsoft Point of Service for .NET from Microsoft 

	website and install.



	http://download.microsoft.com



2.	Download the pole display USB driver from Logic Controls 

	website and install with Device Name driver option.  Refer

	to instructions in the USB driver package for details.



	http://www.logiccontrols.com/web/sd.htm



3.	Connect LD9900U, PD6900U, or PD3900U USB pole display to 

	the USB port of computer.



4.	Invoke Windows Device Manager to verify that the USB driver 

	has been installed properly under Universal Serial Bus 

	controllers with device names \\.\LCLD9\, \\.\LCPD6\ or

	\\.\LCPD3\.



5.	Double click on "PosForNetLDSetup.msi" in this POS for .Net

	driver package to start installation of the driver.  The driver 

	will be installed silently into the following folder:



	c:\Program Files\Logic Controls\USB LineDisplay POS_for_dot_net\



	The driver will be registered in the Widows registry at entry

	\HKLM\SOFTWARE\POSfor.NET\ControlAssemblies.



6.	Invoke CclTestApp.exe in 



	c:\Program Files\Microsoft Point Of Service\SDK Samples\Sample Application\ 



	folder to test and verify installation of the POS for .NET driver.









Logic Controls, Inc.

355 Denton Avenue

New Hyde Park, NY 11040

Tel: (516)-248 0400

Fax: (516)-248 0443

email: lci@logiccontrols.com

web: www.logiccontrols.com

